|  |  |
| --- | --- |
| 0cm – 90cm | Road fill, soil, and fine sand |
| 90cm – 94cm | Stiff, gummy, sandy (fine) clay, light gray with some orangish-brown. |
| 94cm – 130cm | Clean, gray, fine to medium sand with some clay. Absence of clay at bottom. |

Sample: WCA28

